**IOT Flood Monitoring**

* At the start of the system the wifi module is connected to the pre-program SSID and the PASSWORD.
* The pre-program SSID is “**iot**” and the pre-program password is “**project1234**”.
* The user must have to set the above SSID and PASSWORD to his/her router or mobile hotspot.
* All the monitoring data is send over the website <http://iotgecko.com/IOTlogin.aspx>

ID: **abhijeetrtalawar@gmail.com**

Pwd: 4324